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Section 083313
Coiling Counter Doors model 657

NOTE: Enable Microsoft Word option to display hidden text to view notes to specifier.

PART 1 GENERAL
Section Includes
Metal coiling counter doors with integral frame and sill.
Related Requirements
Section << 061000 - Rough Carpentry>>:  Rough openings.
Section << 079200 - Joint Sealants>>:  Sealing joints between frames and adjacent construction.
Section << 087100 - Door Hardware>>:  Cylinder cores and keys.
~~~~~ MASTER NOTE ~~~~~~
This cross-reference is applicable only to doors with electric motor operation.
~~~ END OF MASTER NOTE ~~~~
Section << 260583 - Wiring Connections>>:  Power to disconnect.
Reference Standards
ASTM A240/A240M - Standard Specification for Chromium and Chromium-Nickel Stainless Steel Plate, Sheet, and Strip for Pressure Vessels and for General Applications; 2023a.
ITS (DIR) - Directory of Listed Products; Current Edition.
UL (DIR) - Online Certifications Directory; Current Edition.
~~~~~ MASTER NOTE ~~~~~~
Do not request submittals if drawings sufficiently describe the products of this section or if proprietary specifying techniques are used. The review of submittals increases the possibility of unintended variations from contract documents, thereby increasing the design professional's liability. 
~~~ END OF MASTER NOTE ~~~~
Submittals
Product Data:  Submit manufacturer's standard literature showing materials and details of construction and finish.<<  Include data on electrical operation.; or  None - N/A>>
Shop Drawings:  Indicate rough and actual opening dimensions, anchorage methods, hardware locations, and installation details.
Manufacturer's Instructions:  Indicate installation sequence and installation, adjustment, and alignment procedures.
Installer's qualification statement.
Operation and Maintenance Data:  Indicate modes of operation, lubrication requirements and frequency, and periodic adjustments required.
Specimen warranty.
Quality Assurance
Manufacturer Qualifications:  Company specializing in manufacturing products specified in this section with minimum << three; or  _____>> years of<< documented;    _____; or  None - N/A>> experience.
Installer Qualifications:  Company specializing in performing work of type specified and with minimum << three; or  _____>> years of<<  documented;    _____; or  None - N/A>> experience<< and approved by manufacturer; or  None - N/A>>.
Products Requiring Electrical Connection:  Listed and classified by << ITS (DIR);  UL (DIR);  testing firm acceptable to authorities having jurisdiction; or  _____>> as suitable for purpose specified and indicated.
Delivery, Storage, and Handling
Store products in manufacturer's unopened packaging until ready for installation.
Protect materials from exposure to moisture.
Store materials in dry, warm, ventilated, weathertight location.
Warranty
Manufacturer Warranty:  Provide manufacturer warranty for counterbalance shaft assembly for years indicated under individual doors. Complete forms in <<Owner>>'s name and register with manufacturer.
PART 2 PRODUCTS
Manufacturer
Overhead Door Corporation; www.overheaddoor.com; 1 (800) 929-3667.
Substitutions: Not permitted.
Metal Coiling Counter Doors with Integral Frame and Sill
Overhead DoorTM Brand; Model 657.
Slats:  Interlocking, roll-formed, metal slats.
~~~~~ MASTER NOTE ~~~~~~
Standard maximum width of 12 feet (3658 mm). For larger doors, contact manufacturer.
~~~ END OF MASTER NOTE ~~~~
Width:  << _____ feet (_____ mm)>>.
~~~~~ MASTER NOTE ~~~~~~
Standard maximum height of 4 feet (1219 mm). For larger doors, contact manufacturer.
~~~ END OF MASTER NOTE ~~~~
Height:  << _____ feet (_____ mm)>>.
Mounting:  Between jamb.
Door-Only Warranty:  One year.
Curtain Material:  <<ASTM A240/A240M>>, 300 series stainless steel.
Slat Profile:  << 1-1/4 inch (32 mm)>>, flat.
Endlocks:  Stamped, hot-dip, galvanized endlocks riveted to each end of alternate slats to prevent lateral movement and limit slat deflection and bending stress.
Finish:  No.4 satin.
Bottom Bar:  6063-T6 aluminum.
Finish:  Clear anodized.
Locking Options to Include:  << Best cylinder;  Cylinder;  Slide lock; or  _____>>.
Lock Locations:  << Both jambs;  Left jamb only;  Right jamb only; or  _____>>.
Lock Access:  << Both sides;  Coil side;  Opposite coil side; or  _____>>.
Weatherstripping and Seals:
Bottom Seal Astragal:  << Required;  Not required; or  _____>>.
Guide Seal:  << Brush, one-sided;  Not required; or  _____>>.
Brackets:  Minimum << 12-gauge, 0.1046-inch (2.66 mm)>> steel plate to support counterbalance assembly and form end closures. Provide ball bearings at rotating support points. Bolt plates to mounting structures with minimum << 1/4-inch (6 mm)>> fasteners.
Material:  <<ASTM A240/A240M>>, 300 series stainless steel.
Finish:  No.2B mill finish.
Counterbalance Assembly:  Steel pipe barrel capable of carrying curtain load with maximum deflection of << 0.03-inch per foot (2.5 mm per m)>> of door width.
Material:  Heat-treated helical torsion springs, encased in steel pipe and designed to include overload factor of 25 percent to ensure minimum effort to operate.
Assembly:  Sealed and prelubricated high speed ball bearing at rotating support points. Torsion spring charge wheel for applying spring torque and for future adjustments.
Hood:  <<ASTM A240/A240M>>, << 16-gauge, 0.625-inch (1.587 mm)>> 300 series stainless steel, formed to fit contour of end brackets with reinforced top and bottom edges.
Shape:  Square.
Finish:  No.4 satin.
Integral Frame:  <<ASTM A240/A240M>>, << 16-gauge, 0.625-inch (1.587 mm)>> 300 series stainless steel, with guides incorporated into jamb design, reinforced by << 12-gauge, 0.1046-inch (2.66 mm)>> mounting structure.
Finish:  No.4 satin.
Sill:
Manufacturer's standard sheet metal.
<< 14-gauge, 0.078-inch (1.98 mm)>> stainless steel.
Finish:  No.4 satin.
Not required.
Manual Operation:  << Hand crank;  Push up; or  _____>>.
PART 3 EXECUTION
Examination
Verify adjacent construction is suitable for door installation.
Verify electrical services have been installed and are accessible.
Verify door opening is plumb, header is level, and dimensions are correct.
Notify <<Architect>> of unacceptable conditions or varying dimensions.
Commencement of installation indicates acceptance of substrate and door opening conditions.
Installation
Install units in accordance with manufacturer's instructions.
Use anchorage devices to securely fasten assembly to wall construction and building framing without distortion or stress.
Securely and rigidly brace components suspended from structure.<<  Secure guides to structural members only.;    _____ .; or  None - N/A>>
Fit and align assembly including hardware; level and plumb to provide smooth operation.
Coordinate installation of electrical service; see Section << 260583>>.
Complete wiring from disconnect to unit components.
Complete wiring from fire alarm system.
Install perimeter trim as shown on drawings.

~~~~~ MASTER NOTE ~~~~~~
Limit tolerances to installed dimensions, such as variation in thickness or deviation from intended locations.
~~~ END OF MASTER NOTE ~~~~

Tolerances
Maintain dimensional tolerances and alignment with adjacent work.
Maximum Variation from Plumb:  << 1/16 inch (1.5 mm); or  ___ inch (___ mm)>>.
Maximum Variation from Level:  << 1/16 inch (1.5 mm); or  ___ inch (___ mm)>>.
Longitudinal or Diagonal Warp:  Plus or minus << 1/8 inch per 10 feet (3 mm per 3 m); or  ____ inch per 10 feet (__ mm per 3 m)>> straight edge.
Adjusting
Adjust operating assemblies for smooth and noiseless operation.
Cleaning
See Section << 017000 - Execution and Closeout Requirements>> for additional requirements.
Clean installed components.
Remove labels and visible markings.
END OF SECTION
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