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Section 083313
Coiling Counter Doors model 665

NOTE: Enable Microsoft Word option to display hidden text to view notes to specifier.

PART 1 GENERAL
Section Includes
Wood coiling counter doors.
Related Requirements
Section << 061000 - Rough Carpentry>>:  Rough openings.
Section << 079200 - Joint Sealants>>:  Sealing joints between frames and adjacent construction.
Section << 087100 - Door Hardware>>:  Cylinder cores and keys.
~~~~~ MASTER NOTE ~~~~~~
This cross-reference is applicable only to doors with electric motor operation.
~~~ END OF MASTER NOTE ~~~~
Section << 260583 - Wiring Connections>>:  Power to disconnect.
Reference Standards
ASTM A240/A240M - Standard Specification for Chromium and Chromium-Nickel Stainless Steel Plate, Sheet, and Strip for Pressure Vessels and for General Applications; 2023a.
ITS (DIR) - Directory of Listed Products; Current Edition.
UL (DIR) - Online Certifications Directory; Current Edition.
~~~~~ MASTER NOTE ~~~~~~
Do not request submittals if drawings sufficiently describe the products of this section or if proprietary specifying techniques are used. The review of submittals increases the possibility of unintended variations from contract documents, thereby increasing the design professional's liability. 
~~~ END OF MASTER NOTE ~~~~
Submittals
Product Data:  Submit manufacturer's standard literature showing materials and details of construction and finish.<<  Include data on electrical operation.; or  None - N/A>>
Shop Drawings:  Indicate rough and actual opening dimensions, anchorage methods, hardware locations, and installation details.
Manufacturer's Instructions:  Indicate installation sequence and installation, adjustment, and alignment procedures.
Installer's qualification statement.
Operation and Maintenance Data:  Indicate modes of operation, lubrication requirements and frequency, and periodic adjustments required.
Specimen warranty.
Quality Assurance
Manufacturer Qualifications:  Company specializing in manufacturing products specified in this section with minimum << three; or  _____>> years of<< documented;    _____; or  None - N/A>> experience.
Installer Qualifications:  Company specializing in performing work of type specified and with minimum << three; or  _____>> years of<<  documented;    _____; or  None - N/A>> experience<< and approved by manufacturer; or  None - N/A>>.
Products Requiring Electrical Connection:  Listed and classified by << ITS (DIR);  UL (DIR);  testing firm acceptable to authorities having jurisdiction; or  _____>> as suitable for purpose specified and indicated.
Delivery, Storage, and Handling
Store products in manufacturer's unopened packaging until ready for installation.
Protect materials from exposure to moisture.
Store materials in dry, warm, ventilated, weathertight location.
Warranty
Manufacturer Warranty:  Provide manufacturer warranty for counterbalance shaft assembly for years indicated under individual doors. Complete forms in <<Owner>>'s name and register with manufacturer.
PART 2 PRODUCTS
Manufacturer
Overhead Door Corporation; www.overheaddoor.com; 1 (800) 929-3667.
Substitutions: Not permitted.
Wood Coiling Counter Doors
Overhead DoorTM Brand; Model 665.
Slats:  Interlocking wood slats.
~~~~~ MASTER NOTE ~~~~~~
Standard maximum width of 12 feet (3658 mm). For larger doors, contact manufacturer.
~~~ END OF MASTER NOTE ~~~~
Width:  << _____ feet (_____ mm)>>.
~~~~~ MASTER NOTE ~~~~~~
Standard maximum height of 8 feet (2438 mm). For larger doors, contact manufacturer.
~~~ END OF MASTER NOTE ~~~~
Height:  << _____ feet (_____ mm)>>.
Mounting:  << Surface-mounted on side indicated on drawings;  Between jamb; or  _____>>.
Opening Speed:  Door to operate at variable speed up to << 8 inches (203 mm)>> per second.
Closing Speed:  Door to operate at variable speed up to << 12 inches (305 mm)>> per second.
Available Warranty:
Door-Only Warranty:  One year.
Curtain Material:  Wood; endlocks attached to alternate slats maintain curtain alignment and prevent lateral slat movement.
Slat Profile:  << 1-3/4 inches (16 mm)>> high by << 1/2 inch (13 mm)>> thick.
Wood Species:  << Birch;  Douglas fir;  Red oak;  White oak; or  _____>>.
Finish:  Unfinished.
Bottom Bar:  Wood to match curtain.
Locking Options to Include:  << Cylinder.;  Best cylinder.;  _____ .; or  None - N/A>>
Lock Locations:  << Both jambs;  Left jamb only;  Right jamb only; or  _____>>.
Lock Access:  << Coil side;  Opposite coil side; or  _____>>.
Side Guides, Channels:  Constructed of wood to match curtain.
Brackets:  Galvanized steel to support counterbalance assembly and curtain, covered with wood to match curtain.
Counterbalance Assembly:  Helical-torsion-spring type, housed in steel tube or pipe barrel and supporting curtain with deflection limited to << 0.03 inch per foot (2.5 mm per m)>> of span; adjustable spring tension required.
Hood:  << Not required;  Wood; or  _____>>. 
Finish:  Match curtain.
Manual Operation:  << Push up;  Hand crank; or  _____>>.
~~~~~ MASTER NOTE ~~~~~~
Motor only available on door width greater than 2 feet 6 inches (762 mm) and less than 14 feet (4267 mm), with height no greater than 6 feet (1829 mm).
~~~ END OF MASTER NOTE ~~~~
Motor Operation:  Provide UL-listed electric operator; size as recommended by manufacturer to move door in either direction minimum << 8 inches (203 mm)>> and maximum << 12 inches (305 mm)>> per second.
Manual Override:  Crank.
Operation Supply Voltage:  << 115/208/230 V, 1-phase, 60 Hz;  208/230/460 V, 3-phase, 60 Hz;  220 V, 1-phase, 50 Hz;  220 V, 3-phase, 50 Hz;  400 V, 3-phase, 50 Hz;  575 V, 3-phase, 60 Hz; or  _____>>.
Actuation:  Provide push button.
Motor Mounting:  Within door coil.

PART 3 EXECUTION
Examination
Verify adjacent construction is suitable for door installation.
Verify electrical services have been installed and are accessible.
Verify door opening is plumb, header is level, and dimensions are correct.
Notify <<Architect>> of unacceptable conditions or varying dimensions.
Commencement of installation indicates acceptance of substrate and door opening conditions.
Installation
Install units in accordance with manufacturer's instructions.
Use anchorage devices to securely fasten assembly to wall construction and building framing without distortion or stress.
Securely and rigidly brace components suspended from structure.<<  Secure guides to structural members only.;    _____ .; or  None - N/A>>
Fit and align assembly including hardware; level and plumb to provide smooth operation.
Coordinate installation of electrical service; see Section << 260583>>.
Complete wiring from disconnect to unit components.
Complete wiring from fire alarm system.
Install perimeter trim as shown on drawings.

~~~~~ MASTER NOTE ~~~~~~
Limit tolerances to installed dimensions, such as variation in thickness or deviation from intended locations.
~~~ END OF MASTER NOTE ~~~~

Tolerances
Maintain dimensional tolerances and alignment with adjacent work.
Maximum Variation from Plumb:  << 1/16 inch (1.5 mm); or  ___ inch (___ mm)>>.
Maximum Variation from Level:  << 1/16 inch (1.5 mm); or  ___ inch (___ mm)>>.
Longitudinal or Diagonal Warp:  Plus or minus << 1/8 inch per 10 feet (3 mm per 3 m); or  ____ inch per 10 feet (__ mm per 3 m)>> straight edge.
Adjusting
Adjust operating assemblies for smooth and noiseless operation.
Cleaning
See Section << 017000 - Execution and Closeout Requirements>> for additional requirements.
Clean installed components.
Remove labels and visible markings.
END OF SECTION
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