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Section 083323.13
RAPID Coiling Doors
Model 997

NOTE: Enable Microsoft Word option to display hidden text to view notes to specifier.
	
PART 1 GENERAL
Section Includes
Interior high-speed coiling insulated fabric doors.
Related Requirements
Section 260583 - Wiring Connections:  Power to disconnect.
Reference Standards
ASTM A36/A36M - Standard Specification for Carbon Structural Steel; 2019.
ASTM A500/A500M - Standard Specification for Cold-Formed Welded and Seamless Carbon Steel Structural Tubing in Rounds and Shapes; 2023.
ASTM E330/E330M - Standard Test Method for Structural Performance of Exterior Windows, Doors, Skylights and Curtain Walls by Uniform Static Air Pressure Difference; 2014 (Reapproved 2021).
DASMA 403 - Specification for High Speed Doors and Grilles; 2024.
FBC TAS 201 - Impact Test Procedures; Testing Application Standard; 1994.
FBC TAS 202 - Criteria for Testing Impact and Non-Impact Resistant Building Envelope Components Using Uniform Static Air Pressure; Testing Application Standard; 1994.
ITS (DIR) - Directory of Listed Products; Current Edition.
UL (DIR) - Online Certifications Directory; Current Edition.
~~~~~ MASTER NOTE ~~~~~~
Do not request submittals if drawings sufficiently describe the products of this section or if proprietary specifying techniques are used. The review of submittals increases the possibility of unintended variations from contract documents, thereby increasing the design professional's liability. 
~~~ END OF MASTER NOTE ~~~~
Submittals
Product Data:  Provide << general construction;  electrical equipment;  component connections and details; and  _______>>.
Shop Drawings:  Indicate pertinent dimensioning, anchorage methods, hardware locations, and installation details.
Manufacturer's Instructions:  Indicate installation sequence and procedure details, and adjustment and alignment instructions.
Manufacturer's qualification statement.
Installer's qualification statement.
Maintenance Data:  Indicate << lubrication requirements and frequency;  periodic adjustments required; and  _______>>.
Specimen warranty.
Quality Assurance
Manufacturer Qualifications:  Company specializing in manufacturing products specified in this section, with at least << three; or  _____>> years of<<  documented;    _______; or  None - N/A>> experience.
Installer Qualifications:  Company specializing in performing work of type specified and with at least << three; or  _____>> years<<  documented;    _____; or  None - N/A>> experience<< and approved by manufacturer; or  None - N/A>>.
Products Requiring Electrical Connection:  Listed and classified by << ITS (DIR);  UL (DIR);  testing firm acceptable to authorities having jurisdiction; or  ___>> as suitable for purpose specified.
Delivery, Storage, and Handling
Store products in manufacturer's unopened packaging until ready for installation.
Protect materials from exposure to moisture.
Store materials in dry, warm, ventilated, weathertight location.
Warranty
Manufacturer Warranty:  Provide 5-year manufacturer warranty. Complete forms in <<Owner>>'s name and register with manufacturer.
PART 2 PRODUCTS
Manufacturer
Overhead Door Corporation; www.overheaddoor.com; 1 (800) 929-3667.
Substitutions: Not permitted.
Interior High-Speed Coiling Insulated Fabric Doors
Overhead DoorTM Brand; Model 997 interior high-speed roll-up industrial freezer/cooler door.
Curtain Fabric:  Reinforced, insulated, polyvinyl chloride (PVC) curtain.

~~~~~ MASTER NOTE ~~~~~~
Manufacturer's standard maximum width: 12 feet (3657 mm).
~~~ END OF MASTER NOTE ~~~~

Width:  << ____ feet (____ mm)>>.

~~~~~ MASTER NOTE ~~~~~~
Manufacturer's standard maximum height: 18 feet (5486 mm).
~~~ END OF MASTER NOTE ~~~~

Height:  << ____ feet (____ mm)>>.
Mounting:  Surface-mounted << on side indicated on drawings;  on interior side;  on exterior side; or  _______>>.
Performance Standards:  <<DASMA 403>> requirements for high-performance doors.
Opening Speed:  Door to operate at variable speed up to << 80 inches (2032 mm)>> per second.
Closing Speed:  Door to operate at variable speed up to << 40 inches (1016 mm)>> per second.
Operation Cycles:  Drive motor and gearbox capable of operating for not less than one million cycles. One operation cycle is complete when door is opened from closed position to fully open position and returned to closed position.
Durability:  Doors to operate at minimum of one million cycles when selected, installed, operated, and maintained.
Wind Load:  Design door assembly to withstand ultimate static wind load of << 2 psf (96 Pa)>> in accordance with <<ASTM E330/E330M>>.
Curtain Fabric:  Two layers of PVC-coated polyester with one-ply polyester weave on both interior and exterior side, surrounding overlapping, staggered, insulated sections welded together.
Fabric Color:  << Blue;  Gray;  Red;  White; or  _______>>.
Curtain Retainers:  Nylon 66 curtain lock at outside edges of curtain engaged inside guides under wind load.
Bottom Bar:  Fiber-reinforced composite and two-layer, PVC-coated polyester with one-ply polyester weave wrapped breakaway bottom bar to provide full thermal barrier and strength to break away from either direction, and resettable from either side of opening after impact.
Finish:  Powder-coated << yellow; or  _______>>.
Upon impact, bottom bar releases from guides and door operation stops.
Controller indicates problem encountered and instructs operator on steps to fix problem.
Detection required via solid-state device for accuracy; no external electromechanical switch is allowed.
Press button on control panel to reset door after impact.
Provide door with wireless failsafe electric safety edge.
Include field-adjustable breakaway sensitivity.
Weatherstripping and Seals:  Vinyl brush seal, resilient type, located at guide edges and where curtain enters hood enclosure. Bottom seal is vinyl wrapped, padded bottom bar. Guides have full-height weather seal. No visible air gaps along side or top of door when door panel is in closed or down position.
Side Guides, Channels:  Constructed of high-strength steel with members fully bolted together, combined with composite section interfacing with door to ensure door assembly has full interior-to-exterior thermal barrier.
Actively heated guides ensure complete height of guide has uniform temperature to ensure smooth door movement.

~~~~~ MASTER NOTE ~~~~~~
PowderGuard Premium powder coat in safety yellow is standard. Other options include PowderGuard Premium in black, PowderGuard Premium RAL, and PowderGuard Premium custom color.
~~~ END OF MASTER NOTE ~~~~

Finish:  PowderGuard Premium powder coat in << safety yellow; or  _______>>.
Door Header:  Top-roll assembly fabricated of high-strength steel barrel, supported with powder-coated, high-strength steel brackets at each end with self-aligning bearings.
Drum Barrel System:  <<ASTM A500/A500M>> Grade B, high-strength steel pipe; minimum << 6-5/8-inch (168.3 mm)>> thick.
Brackets:  <<ASTM A36/A36M>> hot-rolled steel with heavy-duty, self-aligning bearings with cast iron housings; minimum << 1/4 inch (6 mm)>> thick.
Springless System:  No balancing springs or counterweights permitted.
Head frame provided with single brush seal along lintel.

~~~~~ MASTER NOTE ~~~~~~
PowderGuard Premium powder coat in black is default finish. Other options include PowderGuard Premium RAL and PowderGuard Premium custom color.
~~~ END OF MASTER NOTE ~~~~

Finish:  PowderGuard Premium powder coat in << black; or  _______>>.
Hood:  << Top-roll assembly enclosed with external metal hood; or  Not required>>.

~~~~~ MASTER NOTE ~~~~~~
Black polyester topcoat is default finish. Other options include PowderGuard PremiumRAL and PowderGuard Premium custom color.
~~~ END OF MASTER NOTE ~~~~

Finish:  << Black polyester topcoat; or  _______>>.
Material:  Galvanized steel with continuous horizontal support.

~~~~~ MASTER NOTE ~~~~~~
Square is typical; sloped is recommended to shed water in exterior or washdown locations.
~~~ END OF MASTER NOTE ~~~~

Shape:  Square.
Motor Cover:  << Not required; or  Required>>.
Steel Finish:  << PowderGuard Premium powder coat;  PowderGuard Zinc base coat with PowderGuard Premium top coat;  PowderGuard Anti-microbial powder coat; or  _______>>.
Obstruction Safety Detection:  Dual infrared sensors mounted in-plane to door curtain at << 18 inches (457 mm)>> and << 50 to 54 inches (1270 to 1372 mm)>> from floor.
Reversing Safety Edge:  Door provided with monitored failsafe electric safety edge. Controller indicates inoperable safety edge.
Wireless connections between safety edge and controller required. No coil cords allowed.
Require ground level replacement of bottom bar wireless system battery.
Operation:  Direct drive motor and gearbox system with field-changeable universal handing and gearbox safety device.
Control Panel:  Variable frequency drive NEMA 4X cULus listed, onboard self-diagnostic and service reminder, built-in padlockable fused disconnect, and easy-to-read LCD text screen for troubleshooting.
Capable of monitoring and reporting on various operating conditions, including current operating status, current command status, current error status, hoist interlock status, service reminder status, and 24 VDC status.
Manual Override:  Pull switch and hand chain allowing manual door operation during power outage and installation.
Limit System:  Magnetic type providing absolute positioning with push-to-set and remote-setting capabilities. Limit system to synchronize with door during manual operation and supply power interruptions.
Timer to Close:  Each door to have automatic closing controlled by adjustable hold-open time delay.

~~~~~ MASTER NOTE ~~~~~~
If project requires a disconnect, select a three-phase power option. If door size is greater than 10 by 10 feet, select three-phase power option.
~~~ END OF MASTER NOTE ~~~~

Operation Supply Voltage:  << 230 VAC three-phase;  460 VAC three-phase;  575 VAC three-phase with transformer; or  _____>>.
Actuation Device Options:  Provide << push button;  key switch;  pull cord;  loop detector;  motion detector;  treadle switch;  radio control;  wireless connection; and  _______>>.
Signaling Device Option:  << Red and green LED warning lights;  Horn and strobe combination;  Rotating warning light; or  _______>>.
Optional LED Lighting System:  Programmable light bar << 3 feet (914 mm)>> tall with red, yellow, green lighting.

~~~~~ MASTER NOTE ~~~~~~
Requirement for air curtain is based on temperature and heat difference between the two sides of the door. Ambient or heated air curtains aid in preventing contaminants moving across opening and drying condensation on curtain. Temperature and humidity measurements will determine if air curtain is needed and if it needs to be ambient or heated. Contact manufacturer to determine if required and which type.
~~~ END OF MASTER NOTE ~~~~

Air Curtain:  << Not required; or  Required. Type:  _______>>.
PART 3 EXECUTION
Examination
Verify << existing conditions; and  _______>> meet manufacturer's requirements before starting work.
Verify opening sizes, tolerances and conditions are acceptable.
Installation
Install in accordance with manufacturer's written instructions.
Use anchorage devices to securely fasten assembly to wall construction and building structure without distortion or stress.
Securely and rigidly brace components suspended from structure.<<  Secure guides to structural members only.;    ______ .; or  None - N/A>>
Fit and align assembly including hardware; level and plumb, to provide smooth operation.
Coordinate installation of electrical service; see Section 260583.
Install enclosure and perimeter trim.
TOLERANCES
Maintain dimensional tolerances and alignment with adjacent work.
Maximum Variation from Plumb:  << 1/16 inch (1.6 mm); or  ___ inch (___ mm)>>.
Maximum Variation from Level:  << 1/16 inch (1.6 mm); or  ___ inch (___ mm)>>.
Longitudinal or Diagonal Warp:  Plus or minus << 1/8 inch per 10 feet (3.2 mm per 3 m); or  ____ inch per 10 feet (____ mm per 3 m)>>.
adjusting
Adjust operating assemblies for smooth and noiseless operation.
CLeaning
See Section 017000 - Execution and Closeout Requirements for additional requirements.
Clean installed components.
Remove labels and visible markings.
PROTECTION
Protect finishes until completion of project.
Touch up damaged finishes after Substantial Completion.
END OF SECTION
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